Team12        Maryville Cyber Team

ccdcadmin1.morainevalley.edu

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Combatants | NISE Username | NISE Password | NETLAB Login (VMs) | Launch Target |
| Darion | team12a | MVcHqFMkam | v12u1 |  |
| Joe | team12b | RTeHjggxRE | v12u2 |  |
| Jonah | team12c | YjJJYqbqqc | v12u3 |  |
| Bradley | team12d | K7Q7rX45T8 | v12u4 |  |
| Connor | team12e | UkrpzzdDZD | v12u5 |  |
| Justin | team12f | XFGDwu6WGE | v12u6 |  |
| Mathew | team12g | QsN3qJZ45C | v12u7 |  |
| Courtney | team12h | Kvf6sJhEuh | v12u8 |  |

Init pwd= ddSv8vVn (delta – delta – SIERRA – victor – Eight -victor -VICTOR - november)

**Required Services**

**HTTP**

Port: 80

**HTTPS**

Port: 443

**SMTP**

Port: 25

**POP3**

Port: 110

**DNS**

DNS lookups will be performed against the DNS server. Each successfully served request will be awarded points.

|  |  |  |
| --- | --- | --- |
| INTERNAL | Local IP | 'Public' IP |
| Docker/Remote | 172.20.240.10 | 172.25.20.12.97 |
| Debian 8.5 DNS/NTP | 172.20.240.20 | 172.25.20.12.20 |
| USER |  |  |
| Ubuntu 14 Web | 172.20.242.10 | 172.25.20.12.23 |
| 2012 AD/DNS/DHCP | 172.20.242.200 | 172.25.12.27 |
| Ubuntu Wkst | dynamic | dynamic |
| PUBLIC |  |  |
| Splunk | 172.20.241.20 | 172.25.20.12.9 |
| CentOS 7 E-Comm | 172.20.241.30 | 172.25.20.12.11 |
| Fedora 21 Webmail/WebApps | 172.20.241.40 | 172.25.20.12.39 |

|  |  |  |  |
| --- | --- | --- | --- |
| Team | Palo Alto e1/3 Outbound to Core | Core connection to Palo Alto | "Public" IP pool |
| 1 | 172.31.21.2/29 | 172.31.21.1 | 172.25.21.0/24 |
| 2 | 172.31.22.2/29 | 172.31.22.1 | 172.25.22.0/24 |
| 3 | 172.31.23.2/29 | 172.31.23.1 | 172.25.23.0/24 |
| 4 | 172.31.24.2/29 | 172.31.24.1 | 172.25.24.0/24 |
| 5 | 172.31.25.2/29 | 172.31.25.1 | 172.25.25.0/24 |
| 6 | 172.31.26.2/29 | 172.31.26.1 | 172.25.26.0/24 |
| 7 | 172.31.27.2/29 | 172.31.27.1 | 172.25.27.0/24 |
| 8 | 172.31.28.2/29 | 172.31.28.1 | 172.25.28.0/24 |
| 9 | 172.31.29.2/29 | 172.31.29.1 | 172.25.29.0/24 |
| 10 | 172.31.30.2/29 | 172.31.30.1 | 172.25.30.0/24 |
| 11 | 172.31.31.2/29 | 172.31.31.1 | 172.25.31.0/24 |
| 12 | 172.31.32.2/29 | 172.31.32.1 | 172.25.32.0/24 |
| 13 | 172.31.33.2/29 | 172.31.33.1 | 172.25.33.0/24 |
| 14 | 172.31.34.2/29 | 172.31.34.1 | 172.25.34.0/24 |
| 15 | 172.31.35.2/29 | 172.31.35.1 | 172.25.35.0/24 |
| 16 | 172.31.36.2/29 | 172.31.36.1 | 172.25.36.0/24 |
| 17 | 172.31.37.2/29 | 172.31.37.1 | 172.25.37.0/24 |
| 18 | 172.31.38.2/29 | 172.31.38.1 | 172.25.38.0/24 |
| 19 | 172.31.39.2/29 | 172.31.39.1 | 172.25.39.0/24 |
| 20 | 172.31.40.2/29 | 172.31.40.1 | 172.25.40.0/24 |

Banner

"UNAUTHORIZED ACCESS TO THIS DEVICE IS PROHIBITED

You must have explicit, authorized permission to access or configure this device.

Unauthorized attempts and actions to access or use this system may result in civil and/or criminal penalties.

All activities performed on this device are logged and monitored."

Password Policy

Minimum length 12 Enforce password history 6

Maximum Age 60 Enable Complexity

Minimum Age 5

Diagram

Description automatically generated

Table

Description automatically generated